\begin{figure}[hb]
    \centering
    \includegraphics[width=0.9\linewidth]{img/EG_CoA_v2.png}
    \caption{\small Color over Angle shown for a 1.56 mm pixel pitch LED panel at 1500 nits, DCI-P3 Gamut and $D_{65}$ white point showing full white without thermal calibration controlled by Brompton S8}
    \label{fig:polarCoA}
\end{figure}%Further we compared the CCT to the reference $D_{65}$ white test pattern as a deltaE-2000 metric, indicating at which angles human eyes would see the color differences of the panel.